**Seminar 7. Multi-module programming in assembly**

* Multi-module programming = building an executable file that is composed from several obj modules.
* You will write several source files: module1.asm, module2.asm … module.asm, compile them separately using the command:

nasm.exe –fobj module1.asm

………..

nasm.exe –fobj moduleN.asm

and link them together in an executable file with the command:

alink.exe -oPE -subsys console -entry start module1.obj module2.obj …moduleN.obj

You will obtain one executable file: module1.exe.

* One module will contain the main program and the other modules describe functions/procedures which are called from the main module.
* At the lab you will only write 2-module programs (one module containing the main program and the other containing a function that is called from the main module.
* Using the reserved word ***global*** we can export a symbol (variable or procedure) defined in the current module, in order to use it in another module; the other module will import the external symbol using the reserved word ***import***.

Obs: Constants/equ can not be exported since they do not have a memory space.

Passing the parameters to a function/procedure defined in another module

There are three alternatives for this:

* Parameters can be passed using the registers; the problem with this is the fact that there is a limited number of registers and some of them can be occupied with data (so they are not available)
* Parameters can be passed to the function in the other module by declaring them global; the problem with this is that it breaks an old and important principle of programming: *modularization* (i.e. a program is better maintained if it is formed by independent modules linked together, e.g. functions, source files etc.) and everything becomes global (part to the same namespace which can cause name clashes – the same symbol is defined in different places); modularization is the reason we have functions with local variables in a program and not the whole code being written in a giant main body/function.
* Parameters can be passed using the stack – this is the most powerful and flexible solution which is used by the majority of compiled programming languages.

Below we will give an example for each of the three mechanisms for passing the parameters described above, all examples solving a simple problem, that of computing the expression: x:=a+b.

**Ex.1.** Parameters are passed by the main module to the function in the other module using registers.

|  |  |
| --- | --- |
| **Module main.asm** | **Module function.asm** |
| **bits 32**  **global start**  **extern exit**  **import exit msvcrt.dll**  **; we import the ‘addition’ function from the**  **; function.asm module**  **extern addition**  **segment data use32 class=data public**  **a db 2**  **b db 3**  **x db 0**  **segment code use32 class=code public**  **start:**  **; put the parameters in registers**  **mov bl, [a]**  **mov bh, [b]**  **; call the function**  **call addition**    **; result is in AL**  **mov [x], al**  **; call exit(0)**  **push dword 0**  **call [exit]** | **bits 32**  **; we export the ‘addition’ function in order to be**  **; used in the main module**  **global addition**  **segment code use32 class=code public**  **; the code segment contains only the addition**  **; function**  **addition:**  **; the parameters are in: BL=a, BH=b**  **; we will return the result in AL**  **mov al, bl**  **add al, bh**  **; return from function**  **; (it removes the Return Address from the stack**  **; and jumps to the Return Address)**  **ret** |

**Ex.2.** Parameters are passed by the main module to the function in the other module using global variables.

|  |  |
| --- | --- |
| **Module main.asm** | **Module function.asm** |
| **bits 32**  **global start**  **extern exit**  **import exit msvcrt.dll**  **; we import the ‘addition’ function from the**  **; function.asm module**  **extern addition**  **; we export variables a, b and x in order to be used**  **; in the other module**  **global a**  **global b**  **global x**  **segment data use32 class=data public**  **a db 2**  **b db 3**  **x db 0**  **segment code use32 class=code public**  **start:**  **; there is no need to do anything with the**  **; parameters. They are already accessible to the**  **; other module (because they are global).**    **; call the function**  **call addition**    **; the result is already placed in x by the addition**  **; function**  **; call exit(0)**  **push dword 0**  **call [exit]** | **bits 32**  **; we export the ‘addition’ function in order to be**  **; used in the main module**  **global addition**  **; import the a, b, x variables from the other module**  **extern a, b, x**  **segment code use32 class=code public**  **; the code segment contains only the addition**  **; function**  **addition:**  **; the parameters are directly accessible in global**  **; variables a, b and x (which are global)**  **mov al, [a]**  **add al, [b]**  **mov [x], al**  **; return from function**  **; (it removes the Return Address from the stack**  **; and jumps to the Return Address)**  **ret** |

**Ex.3.** Parameters are passed by the main module to the function in the other module using the stack.

|  |  |
| --- | --- |
| **Module main.asm** | **Module function.asm** |
| **bits 32**  **global start**  **extern exit**  **import exit msvcrt.dll**  **; we import the ‘addition’ function from the**  **; function.asm module**  **extern addition**  **segment data use32 class=data public**  **a db 2**  **b db 3**  **x db 0**  **segment code use32 class=code public**  **start:**  **; put the parameters a, b and x on the stack**  **; we can not put bytes on the stack, we will put**  **; dwords**  **mov eax, 0**  **mov al, [a]**  **push eax**  **mov al, [b]**  **push eax**  **mov al, [x]**  **push eax**  **; call the function**  **call addition**  **; the result is in the dword from the top of the stack**  **pop eax**  **mov [x], al ; x := a + b**  **; we still have to remove 2 dwords from the stack**  **; (the dwords corresponding to ‘a’ and ‘b’)**  **add esp, 4\*2**  **; instead of the above instruction we could have**  **; used two ‘pop eax’ instructions**  **; call exit(0)**  **push dword 0**  **call [exit]** | **bits 32**  **; we export the ‘addition’ function in order to be**  **; used in the main module**  **global addition**  **segment code use32 class=code public**  **; the code segment contains only the addition**  **; function**  **addition:**  **; the parameters are on the stack**  **; the stack looks like this:**  Return Address  x  b  a  [ESP]  [ESP+4]  [ESP+8]  [ESP+12]    **; remember that a stack element is 4 bytes**  **; (dword) and the stack grows toward smaller**  **; addresses (meaning that the dword from the top**  **; of the stack is placed at the smallest memory**  **; address).**  **; the Return Address was placed on the stack by**  **; the ‘call addition’ instruction in the main module.**  **mov eax, dword [esp+12]**  **mov bl, al ; bl = a**  **mov eax, dword [esp+8]**  **add bl, al ; bl = a + b**  **mov al, bl**  **mov dword [esp+4], eax ; place a+b on the stack**  **; for the main module**  **; return from function**  **; (‘ret’ removes the Return Address from the**  **; top of the stack and jumps to the Return Address)**  **ret** |

**Ex. 4.** Write a program that concatenates 2 strings by calling a function from another module and then prints the resulted string on the screen.

**Main.asm** module:

|  |
| --- |
| bits 32  global start  extern exit, printf  extern concatenare ; import ‘concatenare’ from the other module  import printf msvcrt.dll  import exit msvcrt.dll  segment data use32 class=data public  s1 db 'abcd'  len1 equ $-s1  s2 db '1234'  len2 equ $-s2  s3 times len1+len2+1 db 0  segment code use32 class=code public  start:  ; we place all the parameters on the stack  push dword len1  push dword len2  push dword s3  push dword s2  push dword s1  call concatenare  add esp, 4\*5    push dword s3  call [printf]    push dword 0  call [exit] |

**Function.asm** module:

|  |
| --- |
| bits 32  global concatenare ; export concatenare  segment code use32 class=code public  concatenare:  ; the stack looks like this:  Return Address  s1  s2  s3  [ESP]  [ESP+4]  [ESP+8]  [ESP+12]  len2  len1  [ESP+16]  [ESP+20]  ; first copy s1 in s3  mov esi, [esp+4] ; ESI = the offset of the source string (s1)  mov edi, [esp+12] ; EDI = the offset of the destination string(s3)  mov ecx, [esp+20] ; ECX = len1  cld  rep movsb ; **rep** repeats movsb ECX times    ; then, copy s2 at the end of s3  mov esi, [esp+8] ; ESI = the offset of the source string (s2)  ; EDI already contains the offset of the destination string  mov ecx, [esp+16] ; ECX = len2    rep movsb ; **rep** repeats movsb ECX times    ret |